PRT232 power & pulse cable

Your CBL001 cable is nominally 4 feet (1.2m) long (longer cables are available by special request) and simplifies connection to the Power and Pulse Count terminals when the PRT232 is used in an enclosure.

Receptacle connector		PCB terminal			Wire end
Green/White			J1 (SENSOR)		White=pulse in; Green=Ground
Red/Black			J3			Red=Power+; Black=Ground